DSC 204 F1 Phoenix®
The premium DSC for all requirements
The versatile Premium Differential Scanning Calorimeter, DSC 204 F1 Phoenix®, fascinates with its unique concept: all essential operational components are integrated into the instrument and optional add-ons can be installed anytime on site.

The DSC measuring cell consists of a cylindrical high-conductivity silver block with an embedded heating coil for broad thermal symmetry (3D symmetry) in the sample chamber, the cooling ports for liquid nitrogen or compressed air cooling and a cooling ring for connection of the intracooler (also with simultaneous liquid nitrogen cooling). The gas-tight construction and integrated mass flow controllers for the purge and protective gases allow coupling to an FT-IR or MS for gas analysis.
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