
The Interceptor Class II,A2 and Class II, B2 Biological Safety Cabinets are Kewaunee’s latest design. Developed with comprehensive features created to enhance both safety and ergonomics… the Interceptor leads its class.
Variants		: Class II,A2 / Class II,B2
Certification		: NSF Certified
Filtration		: HEPA
Available Widths	: 1100mm / 1400mm / 1700mm / 2000mm

Class II,A2	: Minimum of 100 FPM (0.5m/s) inflow. HEPA filtered down flow mixed with recycled air. May exhaust some or all HEPA filtered air back into the laboratory.

Class II,B2	: Minimum of 100 FPM (.5m/s) inflow. HEPA filtered, non-recirculated, down flow air. HEPA filtered exhaust air to atmosphere
