Epoxy Resin  (KEMRESIN) 
Work Top material selections are among the most critical of the laboratory furniture decisions. Surfaces must be able to withstand a variety of reagents and caustic substances. Kewaunee Kemresin Work Tops and sinks not only satisfy stringent laboratory requirements, and SEFA 3 performance standards
Physical Properties:
Excellent resistance to practically all acids, alkalies and solvents. Highly resistant to heat and normal physical abuse
Appearance: Ultra-smooth non-porous surface 
Composition: 1” & 3/4" thick molded epoxy resin
 Available Colors: Black, Grey, Slate, Putty
Compliance: SEFA 3 – 2010 Laboratory Work surfaces

